**Minimum Habitability Standards for**

**Permanent Housing: Checklist**

|  |
| --- |
| **About this Tool**  Recipients and subrecipients must document compliance with the applicable standards. Note that these checklists do not cover the requirements to comply with the Lead-Based Paint requirements at §576.403(a). For more discussion about how and when the standards apply, see ***ESG Minimum Standards for Emergency Shelters and Permanent Housing,*** located at <http://OneCPD.info/esg>.  The checklists below offer an optional format for documenting compliance with the appropriate standards. These are intended to:   1. Provide a clear summary of the requirements and an adaptable tool so recipients and subrecipients can formally assess their compliance with HUD requirements, identify and carry out corrective actions, and better prepare for monitoring visits by HUD staff. 2. Provide a tool for a recipient to monitor that its subrecipient is in compliance with HUD requirements. Where non-compliance is identified, the ESG recipient can use this information to require or assist the subrecipient to make necessary changes.   Prior to beginning the review, the subrecipient should organize relevant files and documents to help facilitate their review. For instance, this may include local or state inspection reports (fire-safety, food preparation, building/occupancy, etc.), or policy and procedure documents related to emergency shelter facility maintenance or renovations.  Carefully read each statement and indicate the shelter’s or unit’s status for each requirement (Approved or Deficient). Add any comments and corrective actions needed in the appropriate box. The reviewer should complete the information about the project, and sign and date the form. This template includes space for an “approving official,” if the recipient or subrecipient has designated another authority to approve the review. When the assessment is complete, review it with program staff and develop an action plan for addressing any areas requiring corrective action. |

Minimum Standards for Permanent Housing

**Instructions:** Place a check mark in the correct column to indicate whether the property is approved or deficient with respect to each standard. The property must meet all standards in order to be approved. A copy of this checklist should be placed in the client file.

| **Approved** | **Deficient** | **Standard**  *(24 CFR part 576.403(c))* |
| --- | --- | --- |
|  |  | 1. *Structure and materials*: The structure is structurally sound to protect the residents from the elements and not pose any threat to the health and safety of the residents. |
|  |  | 1. *Space and security*: Each resident is provided adequate space and security for themselves and their belongings. Each resident is provided an acceptable place to sleep. |
|  |  | 1. *Interior air quality*: Each room or space has a natural or mechanical means of ventilation. The interior air is free of pollutants at a level that might threaten or harm the health of residents. |
|  |  | 1. *Water Supply*: The water supply is free from contamination. |
|  |  | 1. *Sanitary Facilities*: Residents have access to sufficient sanitary facilities that are in proper operating condition, are private, and are adequate for personal cleanliness and the disposal of human waste. |
|  |  | 1. *Thermal environment*: The housing has any necessary heating/cooling facilities in proper operating condition. |
|  |  | 1. *Illumination and electricity*: The structure has adequate natural or artificial illumination to permit normal indoor activities and support health and safety. There are sufficient electrical sources to permit the safe use of electrical appliances in the structure. |
|  |  | 1. *Food preparation*: All food preparation areas contain suitable space and equipment to store, prepare, and serve food in a safe and sanitary manner. |
|  |  | 1. *Sanitary condition*: The housing is maintained in sanitary condition. |
|  |  | 1. *Fire safety*: |
|  |  | * 1. There is a second means of exiting the building in the event of fire or other emergency.   2. The unit includes at least one battery-operated or hard-wired smoke detector, in proper working condition, on each occupied level of the unit. Smoke detectors are located, to the extent practicable, in a hallway adjacent to a bedroom.   3. If the unit is occupied by hearing-impaired persons, smoke detectors have an alarm system designed for hearing-impaired persons in each bedroom occupied by a hearing-impaired person.   4. The public areas are equipped with a sufficient number, but not less than one for each area, of battery-operated or hard-wired smoke detectors. Public areas include, but are not limited to, laundry rooms, day care centers, hallways, stairwells, and other common areas. |
|  |  | 11. Meets additional recipient/subrecipient standards (if any). |

# CERTIFICATION STATEMENT

I certify that I have evaluated the property located at the address below to the best of my ability and find the following:

Property meets all of the above standards.

Property does not meet all of the above standards.

**COMMENTS:**

|  |
| --- |
| Recipient Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Subrecipient Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Program Participant Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Street Address: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Apartment: \_\_\_\_\_\_\_\_\_\_\_  City: \_\_\_\_\_\_\_\_\_\_\_ State: \_\_\_\_\_\_\_\_\_\_\_ Zip: \_\_\_\_\_\_\_\_\_\_\_  Evaluator Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date of review: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Evaluator Name: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Approving Official Signature (if applicable): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_  Approving Official Name (if applicable): \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ |